ESP32 + Display TFT 1.4 240x240

Repositorio: → https://github.com/unloquer/ESP32TFT1.4

https://arduino-er.blogspot.com/2020/07/esp32-13-inch-240x240-ips-lcd-st7789.html

https://www.youtube.com/watch?v=PUV9_OdMcCA

7 pins are used to connect to MCU:
# Pin Label Description
;###############################################################
; TFT_eSPI library setting here (no need to edit library files):
;###############################################################
-D USER_SETUP_LOADED=1 ; Set this settings as valid
-D ST7789_DRIVER=1 ; Select ST7789 driver
-D TFT_WIDTH=240 ; Set TFT size
-D TFT_HEIGHT=240
-D TFT_MISO=-1 ; Define SPI pins
-D TFT_MOSI=19 ; SDA marcado en la pantalla
-D TFT_SCLK=18 ; SCL marcado en la pantalla
-D TFT_CS=5
-D TFT_DC=16 ; Data/Comand pin
-D TFT_RST=23 ; Reset pin del ESP32
-D LOAD_GLCD=1 ; Load Fonts
-D SPI_FREQUENCY=40000000 ; Set SPI frequency

Librería - https://github.com/Bodmer/TFT_eSPI/wiki/Installing-on-PlatformIO

Conversores de imágenes → https://duckduckgo.com/?q=UTFT+ImageConverter+565