Software Defined Radio

LimeSDR

3D Design Case https://www.thingiverse.com/thing:2548364

Getting Started

¿Solo tengo 4 antenas, cuáles conectar? → Se conectan como aparece acá https://github.com/myriadrf/LimeSDR-USB_acrylic_case#assembly

https://wiki.myriadrf.org/LimeSDR_Quick_Start

Initial Tests

https://wiki.myriadrf.org/LimeSDR-USB_Quick_Test
https://myriadrf.org/blog/first-tests-limesdr-gqrx/
https://myriadrf.org/blog/limesuite-driver-architecture/
https://github.com/pothosware/SoapySDR/wiki

GQRX

https://discourse.myriadrf.org/t/limesdr-with-gqrx-is-working/314

When using gqrx, specify the args to be “soapy=0,driver=lime”