eMotion

Repositorio https://github.com/unloquer/TalleresESP

¿Qué es el ESP8266? https://www.reddit.com/r/esp8266/wiki/index

Se quiere usar las capacidades inalámbricas del ESP8266 para transmitir señales de control relacionadas con el movimiento y la ubicación. Estas variables de movimiento y ubicación se capturan a través del sensor MPU-60501)https://www.invensense.com/wp-content/uploads/2015/02/MPU-6000-Datasheet1.pdf

Este es un acelerómetro + gyróscopio + procesar digital de movimientos DPM, su funcionamiento es por medio de I2C2)https://en.wikipedia.org/wiki/I ²C , un protocolo digital de comunicación entre periféricos de circuitos embebidos.

https://makerself.wordpress.com/2014/12/19/starting-with-an-accelerometer-mpu-6050-gy-521/

http://fritzing.org/projects/huzzah-esp8266-mpu-6050

https://turnsouthat.wordpress.com/2015/07/31/arduino-mpu6050-getting-ready/ | https://github.com/ezgode/Arduino_MPU6050

http://playground.arduino.cc/Main/MPU-6050

https://www.hackster.io/Aritro/getting-started-with-imu-6-dof-motion-sensor-96e066

Referentes calibracion del sensor

http://42bots.com/tutorials/arduino-script-for-mpu-6050-auto-calibration/

https://www.reddit.com/r/arduino/comments/2lxpl9/help_with_offset_calibration_on_my_mpu6050/

https://www.youtube.com/watch?v=ce3eA8nzInE

3D

http://nikdudnik.com/making-3d-gfx-for-the-cinema-on-low-budget-and-three-js/

https://github.com/facebook/react-vr

https://facebook.github.io/react-vr/docs/input.html#content